**Properties:**

Postcondition testing

1. Check that the measurement in the Z basis after encoding, returns the output of one of the bell states. We expect to measure the output sets to be either, {11,00} and {01,10}, for each message we encode.
2. Check that the decoded message is equal to the message that was encoded